*************************** START ****************************

START TIME: 202205231336

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
chip sync ok
mac l: 0xab37fa84
mac h: 0xa8244c
crc_cal: 168
crc_read: 168
crc_test: 0
ESP32 MAC CRC OK
get mac res: 1
get flash id : 0x0016405e

manufacturer_id: 0x5e

device_id: 0x4016


Wrote 16848 bytes (10926 compressed) at 0x00001000 in 0.1 seconds (effective 941.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (122 compressed) at 0x00008000 in 0.0 seconds (effective 1445.1 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 3799.1 kbit/s)...

Hash of data verified.
Wrote 199280 bytes (103140 compressed) at 0x00010000 in 1.7 seconds (effective 915.8 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 4 s

Download result: PASS

*************************** END ****************************



