*************************** START ****************************

START TIME: 202210091450

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xfae20678
mac h: 0xf412
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 14896 bytes (10242 compressed) at 0x00000000 in 0.1 seconds (effective 935.3 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (128 compressed) at 0x00008000 in 0.0 seconds (effective 6158.8 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 16436.1 kbit/s)...

Hash of data verified.
Wrote 525136 bytes (295842 compressed) at 0x00010000 in 4.3 seconds (effective 978.7 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 6 s

Download result: PASS

*************************** END ****************************



*************************** START ****************************

START TIME: 202210091451

CONNECT BAUD: 115200
set state: ESP_DL_SYNC
serial port opened
-----------
baud:115200
root baud:115200
-------------
===============BAUD : 115200===============CALL DEVICE SYNC
connecting...
mac l: 0xfae20678
mac h: 0xf412
get mac res: 1
get flash id : 0x001840c8

manufacturer_id: 0xc8

device_id: 0x4018


Wrote 14896 bytes (10242 compressed) at 0x00000000 in 0.1 seconds (effective 932.8 kbit/s)...

Hash of data verified.
Wrote 3072 bytes (128 compressed) at 0x00008000 in 0.0 seconds (effective 4106.3 kbit/s)...

Hash of data verified.
Wrote 8192 bytes (47 compressed) at 0x0000e000 in 0.0 seconds (effective 21900.9 kbit/s)...

Hash of data verified.
Wrote 539840 bytes (315944 compressed) at 0x00010000 in 4.6 seconds (effective 929.0 kbit/s)...

Hash of data verified.
Leaving...

com closed
Use time: 7 s

Download result: PASS

*************************** END ****************************



